{"text_format":"3","workbook":"xlsx","n_sheets":6,"sheets":["SFP","SFP+","QSFP","SFP28","连接器","Sheet1"],"not_rendered":{"images":2},"read":"whole","date_system":"1900"}

{"sheet":"SFP","index":0,"n_rows":49,"n_cols":10,"rows_kept":49}
["Part NumberPart Number","Plugable I/O Product Types","Form Factor","Data Rate (Max) (Gb/s)","Installation Type","Port Matrix Configuration","Included Lightpipe","Heat Dissipation Method","Connector Gold Plated","Nickel Plated Shell"]
["WH81-111-00006-1","Cage","SFP","5G","Solder","1 × 1","无","Heat Dissipation Holes","/","/"]
["WH81-111-Y0002-1","Cage","SFP","5G","Press-Fit","1 × 1","无","Heat Dissipation Holes",null,"/"]
["WHSFP00200Y001","Cage","SFP","5G","Press-Fit","1 × 1","  ○  ○","Heat Dissipation Holes","/","/"]
[]
["WHSFP00612W003","Cage","SFP","5G","Press-Fit","1×2","无","Heat Dissipation Holes","/","/"]
["WHSFP00712W008","Cage","SFP","5G","Press-Fit","1×2","  ○  ○","Heat Dissipation Holes","/","/"]
[]
[]
["WHSFP01214W002","Cage","SFP","5G","Solder","1 × 4","无","Heat Dissipation Holes","/","/"]
["WHSFP01314W002","Cage","SFP","5G","Solder","1 × 4","  ○  ○","Heat Dissipation Holes","/","/"]
["WHSFP01014W006","Cage","SFP","5G","Press-Fit","1 × 4","无","Heat Dissipation Holes","/","/"]
["WHSFP01114W002","Cage","SFP","5G","Press-Fit","1 × 4","  ○  ○","Heat Dissipation Holes","/","/"]
[]
[]
[]
["WHSFP01416W009","Cage","SFP","5G","Press-Fit","1 × 6","/","Heat Dissipation Holes","/","Ni 30U"]
["WHSFP01516W002","Cage","SFP","5G","Press-Fit","1 × 6","  ○  ○","Heat Dissipation Holes","/","/"]
[]
["WHSFP05221D018","Cage+Connector","SFP","5G","Press-Fit","2 × 1","▽△▽△","Heat Dissipation Holes","15U","/"]
["WHSFP05121D021","Cage+Connector","SFP","5G","Press-Fit","2 × 1","无","Heat Dissipation Holes","15U","/"]
["WHSFP05221D017","Cage+Connector","SFP","5G","Press-Fit","2 × 1","▽    △","Heat Dissipation Holes","15U","/"]
["WHSFP05221D032","Cage+Connector","SFP","5G","Press-Fit","2 × 1","  △▽","Heat Dissipation Holes","15U","/"]
[]
["WHSFP05422D018","Cage+Connector","SFP","5G","Press-Fit","2 × 2","▽△▽△","Heat Dissipation Holes","15U","/"]
["WHSFP05322D008","Cage+Connector","SFP","5G","Press-Fit","2 × 2","无","Heat Dissipation Holes","15U","/"]
["WHSFP05422D014","Cage+Connector","SFP","5G","Press-Fit","2 × 2","▽    △","Heat Dissipation Holes","15U","/"]
["WHSFP05422D022","Cage+Connector","SFP","5G","Press-Fit","2 × 2","  △▽","Heat Dissipation Holes","15U","/"]
[]
["WHSFP05624D005","Cage+Connector","SFP","5G","Press-Fit","2 × 4","▽△▽△","Heat Dissipation Holes","15U","/"]
["WHSFP05524D003","Cage+Connector","SFP","5G","Press-Fit","2 × 4","无","Heat Dissipation Holes","15U","/"]
["WHSFP05624D012","Cage+Connector","SFP","5G","Press-Fit","2 × 4","▽    △","Heat Dissipation Holes","15U","/"]
["WHSFP05624D006","Cage+Connector","SFP","5G","Press-Fit","2 × 4","  △▽","Heat Dissipation Holes","15U","/"]
[]
["WHSFP05825F008","Cage+Connector","SFP","5G","Press-Fit","2 × 5","▽△▽△","Heat Dissipation Holes","30U","Ni 30U"]
["WHSFP05725F002","Cage+Connector","SFP","5G","Press-Fit","2 × 5","无","Heat Dissipation Holes","30U","Ni 30U"]
["WHSFP05825F009","Cage+Connector","SFP","5G","Press-Fit","2 × 5","▽    △","Heat Dissipation Holes","30U","Ni 30U"]
["WHSFP05825F010","Cage+Connector","SFP","5G","Press-Fit","2 × 5","  △▽","Heat Dissipation Holes","30U","Ni 30U"]
[]
["WHSFP06326F001","Cage+Connector","SFP","5G","Press-Fit","2 × 6","无","Heat Dissipation Holes","30U","Ni 30U"]
["WHSFP06026F042","Cage+Connector","SFP","5G","Press-Fit","2 × 6","▽△▽△","Heat Dissipation Holes","30U","Ni 30U"]
["WHSFP05926F015","Cage+Connector","SFP","5G","Press-Fit","2 × 6","无","Heat Dissipation Holes","30U","Ni 30U"]
["WHSFP06026F043","Cage+Connector","SFP","5G","Press-Fit","2 × 6","▽    △","Heat Dissipation Holes","30U","Ni 30U"]
["WHSFP06026F044","Cage+Connector","SFP","5G","Press-Fit","2 × 6","  △▽","Heat Dissipation Holes","30U","Ni 30U"]
[]
["WHSFP06228F014","Cage+Connector","SFP","5G","Press-Fit","2 × 8","▽△▽△","Heat Dissipation Holes","30U","Ni 30U"]
["WHSFP06128F005","Cage+Connector","SFP","5G","Press-Fit","2 × 8","无","Heat Dissipation Holes","30U","Ni 30U"]
["WHSFP06228F015","Cage+Connector","SFP","5G","Press-Fit","2 × 8","▽    △","Heat Dissipation Holes","30U","Ni 30U"]
["WHSFP06228F016","Cage+Connector","SFP","5G","Press-Fit","2 × 8","  △▽","Heat Dissipation Holes","30U","Ni 30U"]

{"sheet":"SFP+","index":1,"n_rows":48,"n_cols":10,"rows_kept":48}
["Part NumberPart Number","Plugable I/O Product Types","Form Factor","Data Rate (Max) (Gb/s)","Installation Type","Port Matrix Configuration","Included Lightpipe","Heat Dissipation Method","Connector Gold Plated","Nickel Plated Shell"]
["WH81-111-Y0012-1","Cage","SFP+","10G","Press-Fit","1 × 1","无","Heat Dissipation Holes","/","/"]
["WH81-111-Y0017-1","Cage","SFP+","10G","Press-Fit","1 × 1","  ○  ○","Heat Dissipation Holes","/","/"]
["WH81-111-Y0013-1","Cage","SFP+","10G","Solder","1 × 1","无","Heat Dissipation Holes","/","/"]
["WH81-111-Y0018-1","Cage","SFP+","10G","Solder","1 × 1","无","Heat Sink","/","/"]
[]
["WHSFP10612W078","Cage","SFP+","10G","Press-Fit","1 × 2","无","Heat Dissipation Holes","/","Ni 30U"]
["WH81-112-00012-1","Cage","SFP+","10G","Press-Fit","1 × 2","  ○  ○","Heat Dissipation Holes","/","/"]
["WH81-112-00013-1","Cage","SFP+","10G","Press-Fit","1 × 2","无","Heat Sink","/","/"]
[]
["WH81-114-Y0022-1","Cage","SFP+","10G","Press-Fit","1 × 4","无","Heat Dissipation Holes","/","/"]
["WH81-114-Y0006-1","Cage","SFP+","10G","Press-Fit","1 × 4","  ○  ○","Heat Dissipation Holes","/","/"]
["WH81-114-00008-1","Cage","SFP+","10G","Press-Fit","1 × 4","无","Heat Sink","/","/"]
[]
["WHSFP12015W005","Cage","SFP+","10G","Press-Fit","1 × 5","无","Heat Dissipation Holes","/","/"]
[]
["WHSFP11416W010","Cage","SFP+","10G","Press-Fit","1 × 6","无","Heat Dissipation Holes","/","/"]
["WH81-116-Y0019-1","Cage","SFP+","10G","Press-Fit","1 × 6","  ○  ○","Heat Dissipation Holes","/","/"]
[]
["WHSFP15121D002","Cage+Connector","SFP+","10G","Press-Fit","2 × 1","无","Heat Dissipation Holes","15U","/"]
["WHSFP15221D009","Cage+Connector","SFP+","10G","Press-Fit","2 × 1","▽    △","Heat Dissipation Holes","15U","/"]
["WHSFP15221D010","Cage+Connector","SFP+","10G","Press-Fit","2 × 1","  △▽","Heat Dissipation Holes","15U","/"]
["WHSFP15221D008","Cage+Connector","SFP+","10G","Press-Fit","2 × 1","▽△▽△","Heat Dissipation Holes","15U","/"]
[]
["WHSFP15422D008","Cage+Connector","SFP+","10G","Press-Fit","2 × 2","▽△▽△","Heat Dissipation Holes","15U","/"]
["WHSFP15322D002","Cage+Connector","SFP+","10G","Press-Fit","2 × 2","无","Heat Dissipation Holes","15U","/"]
["WHSFP15422D012","Cage+Connector","SFP+","10G","Press-Fit","2 × 2","▽    △","Heat Dissipation Holes","15U","/"]
["WHSFP15422D002","Cage+Connector","SFP+","10G","Press-Fit","2 × 2","  △▽","Heat Dissipation Holes","15U","/"]
[]
["WHSFP15624D003","Cage+Connector","SFP+","10G","Press-Fit","2 × 4","▽△▽△","Heat Dissipation Holes","15U","/"]
["WHSFP15624D008","Cage+Connector","SFP+","10G","Press-Fit","2 × 4","▽    △","Heat Dissipation Holes","15U","/"]
["WHSFP15624D009","Cage+Connector","SFP+","10G","Press-Fit","2 × 4","  △▽","Heat Dissipation Holes","15U","/"]
["WHSFP15524D002","Cage+Connector","SFP+","10G","Press-Fit","2 × 4","无","Heat Dissipation Holes","15U","/"]
[]
["WHSFP15825F012","Cage+Connector","SFP+","10G","Press-Fit","2 × 5","▽△▽△","Heat Dissipation Holes","30U","/"]
["WHSFP15725F005","Cage+Connector","SFP+","10G","Press-Fit","2 × 5","无","Heat Dissipation Holes","30U","/"]
["WHSFP15825F013","Cage+Connector","SFP+","10G","Press-Fit","2 × 5","▽    △","Heat Dissipation Holes","30U","/"]
["WHSFP15825F014","Cage+Connector","SFP+","10G","Press-Fit","2 × 5","  △▽","Heat Dissipation Holes","30U","/"]
[]
["WHSFP16026F033","Cage+Connector","SFP+","10G","Press-Fit","2 × 6","▽△▽△","Heat Dissipation Holes","30U","Ni 30U"]
["WHSFP15926F008","Cage+Connector","SFP+","10G","Press-Fit","2 × 6","无","Heat Dissipation Holes","30U","Ni 30U"]
["WHSFP16026F034","Cage+Connector","SFP+","10G","Press-Fit","2 × 6","▽    △","Heat Dissipation Holes","30U","Ni 30U"]
["WHSFP16026F108","Cage+Connector","SFP+","10G","Press-Fit","2 × 6","  △▽","Heat Dissipation Holes","30U","Ni 30U"]
[]
["WHSFP16228F028","Cage+Connector","SFP+","10G","Press-Fit","2 × 8","▽△▽△","Heat Dissipation Holes","30U","Ni 30U"]
["WHSFP16128F007","Cage+Connector","SFP+","10G","Press-Fit","2 × 8","无","Heat Dissipation Holes","30U","Ni 30U"]
["WHSFP16228F024","Cage+Connector","SFP+","10G","Press-Fit","2 × 8","▽    △","Heat Dissipation Holes","30U","Ni 30U"]
["WHSFP16228F015","Cage+Connector","SFP+","10G","Press-Fit","2 × 8","  △▽","Heat Dissipation Holes","30U","Ni 30U"]

{"sheet":"QSFP","index":2,"n_rows":0,"n_cols":0,"rows_kept":0}

{"sheet":"SFP28","index":3,"n_rows":74,"n_cols":10,"rows_kept":74}
["Part NumberPart Number","Plugable I/O Product Types","Form Factor","Data Rate (Max) (Gb/s)","Installation Type","Port Matrix Configuration","Included Lightpipe","Heat Dissipation Method","Connector Gold Plated","Nickel Plated Shell"]
["WHSFP30211W037","Cage","SFP28","25G","Press-Fit","1 × 1","/","Heat Dissipation Holes","/","/"]
["WHSFP30211W018","Cage","SFP28","25G","Press-Fit","1 × 1","无","Heat Sink","/","/"]
["WHSFP30311W002","Cage","SFP28","25G","Press-Fit","1 × 1","  ○  ○","Heat Dissipation Holes","/","/"]
[]
[]
["WHSFP30412W009","Cage","SFP28","25G","Press-Fit","1 × 2","无","Heat Dissipation Holes","/","/"]
["WHSFP30412W012","Cage","SFP28","25G","Press-Fit","1 × 2","无","Heat Dissipation Holes","/","/"]
[]
["WHSFP30614W039","Cage","SFP28","25G","Press-Fit","1 × 4","无","Heat Dissipation Holes","/","/"]
["WH81-164-00020-1","Cage","SFP28","25G","Press-Fit","1 × 4","无","Heat Dissipation Holes","/","/"]
["WH81-114-Y0010-1","Cage+Gasket","SFP28","25G","Press-Fit","1 × 4","无","Heat Dissipation Holes","/","/"]
[]
[]
["WHSFP30816W010","Cage","SFP28","25G","Press-Fit","1 × 6","无","Heat Sink散热器","/","/"]
[]
[]
["WHSFP32221F013","Cage+Connectors","SFP28","25G","Press-Fit","2 × 1","  ","Heat Dissipation Holes散热孔","/","/"]
["WHSFP32321F004","Cage+Connectors","SFP28","25G","Press-Fit","2 × 1","△     ▽","Heat Dissipation Holes","/","/"]
["WHSFP32221F005","Cage+Connectors","SFP28","25G","Press-Fit","2 × 1","   ▽△","Heat Dissipation Holes","/","/"]
["WHSFP32121F004","Cage+Connectors","SFP28","25G","Press-Fit","2 × 1","△ ▽△▽","Heat Dissipation Holes","/","/"]
["WHSFP32521F002","Cage+Connectors","SFP28","25G","Press-Fit","2 × 1","  △£▽","Heat Dissipation Holes","/","/"]
["WHSFP32321F002","Cage+Connectors","SFP28","25G","Press-Fit","2 × 1","▽      △ ","Heat Dissipation Holes","/","/"]
["WHSFP32221F003","Cage+Connectors","SFP28","25G","Press-Fit","2 × 1","   △▽","Heat Dissipation Holes","/","/"]
["WHSFP32121F002","Cage+Connectors","SFP28","25G","Press-Fit","2 × 1"," ▽△▽△","Heat Dissipation Holes","/","/"]
["WHSFP32021F003","Cage+Connectors","SFP28","25G","Press-Fit","2 × 1","/","Heat Dissipation Holes","/","/"]
[]
["WHSFP32222F008","Cage+Connectors","SFP28","25G","Press-Fit","2 × 2","  ","Heat Dissipation Holes","/","/"]
["WHSFP32322F006","Cage+Connectors","SFP28","25G","Press-Fit","2 × 2","△     ▽","Heat Dissipation Holes","/","/"]
["WHSFP32221F005","Cage+Connectors","SFP28","25G","Press-Fit","2 × 2","   ▽△","Heat Dissipation Holes","/","/"]
["WHSFP32122F005","Cage+Connectors","SFP28","25G","Press-Fit","2 × 2","△ ▽△▽","Heat Dissipation Holes","/","/"]
["WHSFP32522F002","Cage+Connectors","SFP28","25G","Press-Fit","2 × 2","  △£▽","Heat Dissipation Holes","/","/"]
["WHSFP32322F002","Cage+Connectors","SFP28","25G","Press-Fit","2 × 2","▽      △ ","Heat Dissipation Holes","/","/"]
["WHSFP32222F003","Cage+Connectors","SFP28","25G","Press-Fit","2 × 2","   △▽","Heat Dissipation Holes","/","/"]
["WHSFP32122F002","Cage+Connectors","SFP28","25G","Press-Fit","2 × 2"," ▽△▽△","Heat Dissipation Holes","/","/"]
["WHSFP32022F002","Cage+Connectors","SFP28","25G","Press-Fit","2 × 2","/","Heat Dissipation Holes","/","/"]
[]
["WHSFP32424F004","Cage+Connectors","SFP28","25G","Press-Fit","2 × 4","  ▽○△","Heat Dissipation Holes","/","/"]
["WHSFP32424F002","Cage+Connectors","SFP28","25G","Press-Fit","2 × 4","  △○▽","Heat Dissipation Holes","/","/"]
["WHSFP32224F007","Cage+Connectors","SFP28","25G","Press-Fit","2 × 4",null,"Heat Dissipation Holes","/","/"]
["WHSFP32324F005","Cage+Connectors","SFP28","25G","Press-Fit","2 × 4","△     ▽","Heat Dissipation Holes","/","/"]
["WHSFP32324F006","Cage+Connectors","SFP28","25G","Press-Fit","2 × 4","△     ▽","Heat Dissipation Holes","/","/"]
["WHSFP32024F003","Cage+Connectors","SFP28","25G","Press-Fit","2 × 4","/","Heat Dissipation Holes","/","/"]
["WHSFP32524F004","Cage+Connectors","SFP28","25G","Press-Fit","2 × 4","  ▽£△","Heat Dissipation Holes","/","/"]
["WHSFP32524F002","Cage+Connectors","SFP28","25G","Press-Fit","2 × 4","  △□▽","Heat Dissipation Holes","/","/"]
["WHSFP32324F002","Cage+Connectors","SFP28","25G","Press-Fit","2 × 4","▽      △ ","Heat Dissipation Holes","/","/"]
["WHSFP32224F002","Cage+Connectors","SFP28","25G","Press-Fit","2 × 4","    △▽","Heat Dissipation Holes","/","/"]
["WHSFP32124F002","Cage+Connectors","SFP28","25G","Press-Fit","2 × 4"," ▽△▽△","Heat Dissipation Holes","/","/"]
["WHSFP32024F002","Cage+Connectors","SFP28","25G","Press-Fit","2 × 4","/","Heat Dissipation Holes","/","/"]
[]
["WHSFP32426F002","Cage+Connectors","SFP28","25G","Press-Fit","2 × 6","  △○▽","Heat Dissipation Holes","/","/"]
["WHSFP32226F006","Cage+Connectors","SFP28","25G","Press-Fit","2 × 6",null,"Heat Dissipation Holes","/","/"]
["WHSFP32126F004","Cage+Connectors","SFP28","25G","Press-Fit","2 × 6","△ ▽△▽","Heat Dissipation Holes","/","/"]
["WHSFP32326F004","Cage+Connectors","SFP28","25G","Press-Fit","2 × 6","△     ▽","Heat Dissipation Holes","/","/"]
["WHSFP32226F004","Cage+Connectors","SFP28","25G","Press-Fit","2 × 6","   ▽△","Heat Dissipation Holes","/","/"]
["WHSFP32526F002","Cage+Connectors","SFP28","25G","Press-Fit","2 × 6","  △□▽","Heat Dissipation Holes","/","/"]
["WHSFP32326F002","Cage+Connectors","SFP28","25G","Press-Fit","2 × 6","▽      △ ","Heat Dissipation Holes","/","/"]
["WHSFP32226F002","Cage+Connectors","SFP28","25G","Press-Fit","2 × 6","   △▽","Heat Dissipation Holes","/","/"]
["WHSFP32126F002","Cage+Connectors","SFP28","25G","Press-Fit","2 × 6"," ▽△▽△ ","Heat Dissipation Holes","/","/"]
["WHSFP32026F002","Cage+Connectors","SFP28","25G","Press-Fit","2 × 6","/","Heat Dissipation Holes","/","/"]
[]
["WHSFP32328F003","Cage+Connectors","SFP28","25G","Press-Fit","2 × 8","△     ▽","Heat Dissipation Holes","/","/"]
["WHSFP32028F002","Cage+Connectors","SFP28","25G","Press-Fit","2 × 8","/","Heat Dissipation Holes","/","/"]
["WHSFP32128F002","Cage+Connectors","SFP28","25G","Press-Fit","2 × 8"," ▽△▽△","Heat Dissipation Holes","/","/"]
["WHSFP32228F002","Cage+Connectors","SFP28","25G","Press-Fit","2 × 8","   △▽","Heat Dissipation Holes","/","/"]
["WHSFP32328F002","Cage+Connectors","SFP28","25G","Press-Fit","2 × 8","▽      △ ","Heat Dissipation Holes","/","/"]
["WHSFP32528F002","Cage+Connectors","SFP28","25G","Press-Fit","2 × 8","  △□▽","Heat Dissipation Holes","/","/"]
[]
["WHSFP3232CF003","Cage+Connectors","SFP28","25G","Press-Fit","2 × 12","△     ▽","Heat Dissipation Holes","/","/"]
["WHSFP3222CF004","Cage+Connectors","SFP28","25G","Press-Fit","2 × 12",null,"Heat Dissipation Holes","/","/"]
["WHSFP3232CF002","Cage+Connectors","SFP28","25G","Press-Fit","2 × 12","▽      △ ","Heat Dissipation Holes","/","/"]
["WHSFP3222CF002","Cage+Connectors","SFP28","25G","Press-Fit","2 × 12","   △▽","Heat Dissipation Holes","/","/"]
["WHSFP3212CF002","Cage+Connectors","SFP28","25G","Press-Fit","2 × 12"," ▽△▽△","Heat Dissipation Holes","/","/"]
["WHSFP3202CF002","Cage+Connectors","SFP28","25G","Press-Fit","2 × 12","/","Heat Dissipation Holes","/","/"]

{"sheet":"连接器","index":4,"n_rows":7,"n_cols":10,"rows_kept":7}
["Part NumberPart Number","Plugable I/O Product Types","Form Factor","Data Rate (Max) (Gb/s)","Installation Type","Port Matrix Configuration","Included Lightpipe","Heat Dissipation Method","Connector Gold Plated","Nickel Plated Shell"]
["WH81-151-Y0002-1","Connectors","/","10G","SMD","1 × 1","无","无","15U","/"]
[]
["WHSFP30111D002","Connectors","/","25G","SMD","1 × 1","无","无","15U","/"]
["WHSFP30111F002","Connectors","/","25G","SMD","1 × 1","无","无","30U","/"]
[]
["WHSFP20311D005","Connectors","/","40G","SMD","1 × 1","无","无","15U","/"]

{"sheet":"Sheet1","index":5,"n_rows":0,"n_cols":0,"rows_kept":0}